{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["TR23"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":33,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"TR23","index":0,"n_rows":56,"n_cols":23,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[null,null,null,"LOCALITA'",{"$nulls":7},"LOCALITA'",{"$nulls":8},"Frequenza di calcolo"]
[null,null,null,"A",null,null,null,"Grad","Prad","Srad","GTOTrad","B",null,null,null,"Grad","Prad","Srad","GTOTrad"]
[null,null,null,"AAAAAAAAA",{"$nulls":7},"BBBBBBBBBBB",{"$nulls":8},7400,"MHz"]
[{"$nulls":10},"lambdaA",{"$nulls":7},"lambaB"]
[null,"LONG. (EGw)",null,120000,12,0,0,0.20943951023931953,0,0,0.20943951023931953,130305,13,3,5,0.22689280275926282,0.0008726646259971647,2.42406840554768e-05,0.22778970806931548,"(GG.PP.SS.)"]
[null,"LAT. (N)",null,452900,45,29,0,0.7853981633974483,0.008435758051305926,0,0.7938339214487542,453100,45,31,0,0.7853981633974483,0.00901753446863737,0,0.7944156978660857,"(GG.PP.SS.)"]
[null,"h s.l.m. (m)",null,2,{"$nulls":6},"fiA",2,{"$nulls":6},"fiB"]
[null,"altezza ant. da terra (m)",null,43.5,{"$nulls":6},"fiA",43,{"$nulls":7},"(la più alta / higher)"]
[null,"altezza totale (m)",null,45.5,{"$nulls":6},"fiA",45]
[{"$nulls":7},"diff_angAB","somm_angAB"]
[null,"AZIMUT (°N)",null,87.0352319025103,null,null,null,-0.045200730944976134,1.5642520928805892,null,null,267.7851458693827,null,null,null,"KmAB","deltahAB","elevazAB","elevazBA"]
[null,"ELEVAZ. (°)",null,-0.27697580542749917,{"$nulls":7},-0.27627720344555967,null,null,null,82.0129994463283,395.9653892180208,-0.00483413975307304,-0.004821946848327238,"zenith"]
[]
[null,"dist. effettiva",null,82.0129994463283,null,null,"KmassAB",82.0129994463283,null,null,null,"Km",{"$nulls":7},"effective lenght"]
[]
[null,"CONFIG.:",null,1,{"$nulls":7},1]
[null,"su:",null,1,{"$nulls":7},2]
[null,"tipo antenna",null,1.8,{"$nulls":7},2.4,{"$nulls":7},"type antennas"]
[null,"G. ant. (dB)",null,39.89371139162809,{"$nulls":7},42.392486123794086]
[]
[null,"tipo cavi (feeder)",null,"FLEX GUIDA",{"$nulls":7},"FLEX GUIDA"]
[null,"L cavi (m)",{"$nulls":17},"lenght"]
[null,"A cavi (dB)",null,1.4,{"$nulls":7},0.8,{"$nulls":7},"attenuation"]
[]
[null,"Ao (dB)",null,148.20228830579592]
[null,"Asuppl.(dB)"]
[null,"Atot. (dB)",null,148.20228830579592]
[]
[null,"tratta (path)",null,"16 x 2 Mb/s"]
[null,"Ptx (dBm)",null,28]
[]
[null,"PRx all'antenna (dBm)",null,-38.71609079037374,{"$nulls":7},-40.916090790373744]
[null,"Tipo Accoppiatore",null,"A",{"$nulls":15},"(Power splitter - Simm. - Asimm.)"]
[null,"perdite tot. Accopp. e  guide",null,3,{"$nulls":7},0.8]
[null,"Prx effettiva",null,-41.71609079037374,{"$nulls":7},-41.71609079037374,{"$nulls":7},"effective PRx at receiver"]
[null,"soglia (dbm) 10-3",null,-81,{"$nulls":7},-81,{"$nulls":7},"threshold receiver"]
[null,"Margine BER 10-3:",null,39.28390920962626,{"$nulls":7},39.28390920962626]
[]
[null,"Space diversity",{"$nulls":4},"semplice","calcolo div.","risultato div.",null,null,10]
[null,"Outage BER 10-3",null,6.103209373662589e-05,null,null,6.103209373662589e-05,0,{"$error":"#DIV/0!"},null,null,6.647174466383917e-07,null,null,6.103209373662589e-05,91.8165967288467,6.647174466383917e-07,null,null,"(Morita/Vigant)"]
[null,"equivalent to availability:",null,0.9999389679062634,{"$nulls":7},0.9999993352825534,{"$nulls":7},"deep Fading availability"]
[null,"Outage objectives CCIR:",null,1.771480788040691e-05,{"$nulls":7},1.771480788040691e-05,{"$nulls":7},"(proportional to distance)"]
[]
[null,null,null,"                            GAMMA Tx"]
[null,null,null,"AAAAAAAAA",{"$nulls":7},"BBBBBBBBBBB",{"$nulls":9},"(f1/f2 = MHz )"]
[null,null,"X","ALTA (high)",{"$nulls":7},"BASSA",{"$nulls":8},"CAN. 1",null,"7121/7317"]
[null,null,null,"BASSA (low)",{"$nulls":7},"ALTA",{"$nulls":8},"CAN. 2",null,"7149/7345"]
[null,null,null,"half-band Tx",null,"FREQUENZE",{"$nulls":14},"CAN. 3",null,"7177/7373"]
[{"$nulls":20},"CAN. 4",null,"7205/7401"]
[{"$nulls":19},"X","CAN. 5",null,"7233/7429"]
[{"$nulls":11},"Polarizz.",{"$nulls":8},"CAN. 6",null,"7625/7475"]
[{"$nulls":20},"CAN. 7",null,"7653/7485"]
[{"$nulls":20},"CAN. 8",null,"7681/7513"]
[{"$nulls":20},"CAN. 9",null,"7709/7541"]
["NOTE:",{"$nulls":19},"CAN. 10",null,"7737/7569"]